MSTS Conrail B40-8 #5068 
by The Keystone Works
========================
Installation:

    1.  Unzip the contents of this file to your Trainset folder
    (Drive:\Program Files\Microsoft Games\Train Simulator\Trains\Trainset)

    2.  Create a consist and enjoy!!

------------------------------------------

Credits:

Textures: Pete Willard, John Peterson, John Rosh
Physics:     Bob Boudoin
3D model:    Pete Willard
3D Coupler:  Larry Goss

------------------------------------------
The GE B40-8, a modern diesel-electric locomotive, most effective  
pulling intermodal freight over long stretches at high speeds.   
Locomotive type: Diesel-Electric   
Power: 4,000 hp   
Max. speed: 75 mph (119 km/h)   
Gear ratio: 81:22   
Power source: Diesel engine 7FDL16   
Alternator: GMG 192   
Traction motors: Four 752AH electric motors   
Max. starting tractive effort: 98,961 lb (44,889 kg)   
Max. continuous tractive effort: 69,200 lb (31,389 kg)   
Wheel configuration: Eight 42-inch diameter in B-B configuration 
 (Two sets of two driven axles)   

Height: 15 ft. 6 in. (4.724 m)   
Width: 10 ft. 3 in. (3.1 m)   
Length: 66 ft. 4 in.   
Weight: 144.1 U.S. tons (130.7 metric tons)	

------------------------------------------

The Keystone Works makes no guarantee/warranty about the performance of the 
software included within this archive, implied or otherwise.  Use of this 
software is at your own risk.  The Keystone Works is not responsible for any 
damages that may result from the use of this software.

These files may not be distributed or re-distributed via any other medium 
other than www.train-sim.com or www.trainsimstuff.com without the express 
written consent of The Keystone Works and the original authors.

These files may be freely distributed as long as this readme is included 
UNCHANGED.  If you would like to repaint/reskin, just let us know as we may 
be interested in them too.


Any questions or comments, feel free to email me, 
 Pete Willard @ pwillard@mindspring.com

© Copyright 2003 The Keystone Works